 Break down Salient Characteristics and Specs absolutely needed to fulfill the requirement. 

 Below is a breakdown of all mandatory rental equipment for Phase 1 of the Antenna Farm Project.
	ITEM
NUMBER
	Description
	QUANTITY
	UNIT

	0001
	One (1) Excavator (Caterpillar 320/323 or equivalent)
· Operating Weight: Minimum of 49,500 lbs to 55,100 lbs.
· Engine Power: Minimum of 170 Net Horsepower (HP).
· Reach and Depth: Must be configured to provide a minimum maximum reach of 35' 2" and a maximum digging depth of 25' 1".
· Attachment Requirement: Must include one (1) B-Linkage Grubber attachment (Model B GRUB24 or equivalent) compatible with the excavator's hydraulic and mounting system.
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	0002
	One (1) Compact Track Loader (Caterpillar 299D3 C3H2 or equivalent)
· Operating Weight: Minimum of 11,400 lbs.
· Engine Power: Minimum of 98 Gross Horsepower (HP).
· Rated Operating Capacity (35% Tipping Load): Minimum of 3,480 lbs.
· Cab Configuration: Must include an enclosed cab (ROPS/FOPS) with functional air conditioning and heating.
	1
	EA

	0003
	One (1) Compact Track Loader (Caterpillar 299D3 C3H2 or equivalent)
· Operating Weight: Minimum of 11,400 lbs.
· Engine Power: Minimum of 98 Gross Horsepower (HP).
· Rated Operating Capacity (35% Tipping Load): Minimum of 3,480 lbs.
· Cab Configuration: Must include an enclosed cab (ROPS/FOPS) with functional air conditioning and heating.
	1
	EA



