Bill of Materials for Rudder Seal Kit
NSN 5330-01-565-8083
P/N 225WLB-562-003 SEAL KIT

LIP SEAL, 16" X 17" X .350" NOMINAL SIZE, SKF P/N HD1 NO. 511202, ALTERNATE P/N MMC P/N 80195-00 OR EQUAL, QUANTITY 1 EACH.

LIP  SEAL, 16" X 17.5" X .875" NOMINAL SIZE, SKF P/N HDSA2 NO. 1600926, ALTERNATE P/N MMC P/N 81095-002 OR EQUAL, QUANTITY 1 EACH. 

GASKET, COMMERICAL GRADE 1/16" THICK NEOPRENE RUBBER, 70 DUROMETER SHORE A+/-5, DIMENSIONS: 25" OD X 18.75" ID NOMINAL SIZE.  BOLTS HOLES: EIGHT EACH  11/16" DIAMETER ON 22.62"  BOLT CIRCLE EQUALLY SPACED,  MMC P/N 81079-002  OR EQUAL. QUANTITY 1 EACH.

GASKET, COMMERICAL GRADE 1/16" THICK NEOPRENE RUBBER, 70 DUROMETER SHORE A+/-5, DIMENSIONS: 25" OD X 18.62" ID NOMINAL SIZE.  BOLTS HOLES: EIGHT EACH  25/64" DIAMETER ON 22.00"  BOLT CIRCLE EQUALLY SPACED,  MMC P/N  81079-003 OR EQUAL. QUANTITY 1 EACH.

GASKET, COMMERICAL GRADE 1/16" THICK NEOPRENE RUBBER, 70 DUROMETER SHORE A +/-5,
DIMENSIONS: 35" OD X 30" ID NOMINAL SIZE, BOLT HOLES: EIGHT EACH 1 1/16" ON 32.00 BOLT CIRLE, MMC P/N 81079-001 OR EQUAL, QUANTITY 1 EACH

O-RING, BUNA-N, SHORE A HARNESS 70 DUR0METER, DIMENSIONS: 19.50" X 18.50" X .50" NOMINAL. JOINING ENDS TO BE VULCANIZED, MMC P/N 81096-004 OR EQUAL. QUANTITY 1 EACH.

O-RING, BUNA-N, SHORE A HARNESS 70 DUR0METER, DIMENSIONS: 19.00" X 18.50" X .25" NOMINAL. JOINING ENDS TO BE VULCANIZED, MMC P/N 81096-003 OR EQUAL. QUANTITY 1 EACH.

O-RING, BUNA-N, SHORE A HARNESS 70 DUR0METER, DIMENSIONS: 19.00" X 18.00" X .50" NOMINAL. JOINING ENDS TO BE VULCANIZED, MMC P/N 81096-002 OR EQUAL. QUANTITY 1 EACH.   
        
O-RING, BUNA-N, SHORE A HARNESS 70 DUR0METER, DIMENSIONS: 14.50" X 14.00" X .25" NOMINAL. JOINING ENDS TO BE VULCANIZED, MMC P/N 81096-001 OR EQUAL. QUANTITY 1 EACH.
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