Specification 
26 May 2026

PICKUP TRUCK, 4 DOOR

THE TRUCK SHALL BE PROVIDED WITH ALL NEW PARTS, THE MANUFACTURER’S STANDARD EQUIPMENT, AND THE FOLLOWING MINIMUM EQUIPMENT AND CAPABILITIES:

1. CONFIGURATION
1.1. The vehicle shall be a Ford F-350 Crew Cab (4-door) Pickup Truck.
1.2. The vehicle shall have a 4x4 drivetrain and have dual rear wheels (DRW or dually). 
1.3. ULSD diesel engine
1.4. The vehicle shall be left-hand drive (LHD).
1.5. The vehicle shall be a 2026 model year or later with no more than 500 miles (804.6 km) on the odometer when delivered.
1.6. The vehicle shall be able to tow a 35,000 lb (15,876 kg) trailer.
1.7. The exterior of the vehicle shall be OEM color.

2. EQUIPMENT
2.1. The Pickup shall be equipped with all standard equipment and the options specified herein.
2.2. A limited slip rear differential shall be provided.
2.3. Vehicle shall be equipped with a 40,000 lb. (18,143 kg) GTWR ball hitch, mounted in the bed, suitable for a gooseneck trailer.
2.3.1. SAE J560 7 pin, 12 volt connector for trailer connection
2.4. Front and rear tow hooks shall be provided for vehicle recovery.
2.5. Air conditioning shall be provided.
2.6. A brushguard with integrated headlight protection shall be provided.
2.7. Front and rear anti-sail mud flaps shall be provided.
2.8. The vehicle shall be provided with front row rubber floor mats.
2.9. Safety equipment 
2.9.1. An ABC type fire extinguisher, minimum 2.2 lb (1.0 kg) capacity, with mounting bracket 
2.9.2. A first aid kit, three triangles, and tow rope
2.9.3. A portable 12 volt air compressor kit with pump, hose, and fittings
2.9.4. Storage for the first aid kit, triangles, tow rope, and portable 12 volt air compressor kit
2.10. Vehicle language requirements: 
2.10.1. All instructions, diagrams, and warning labels shall be in English, or in universal symbols, and shall be permanently affixed to the vehicle.  
2.10.2. Fuel filler cap or area near the cap shall be labeled with the type of fuel compatible with the vehicle in English or in universal symbols. 
2.10.3. A manual(s) shall be provided with every vehicle and written in English.

3. WHEEL ASSEMBLY (TIRE AND WHEEL)
3.1. The vehicle shall be provided with all-terrain tires.
3.2. The vehicle shall be provided with a full-size spare wheel assembly with holder.   
3.3. All tires shall be of the same size, load rating and tread design, and all wheel assemblies shall be interchangeable, including the spare wheel assembly.
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