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THIS EQUIPMENT CONFORMS
WITH CARRIER ENGINEERING
REQUIREMENT Z-420

Rockwell
Automation

ID No:180700-A05-50C
Input Rating:380-480VAC 608A 50/60Hz 3PH

Output Rating:0-480VAC 608A 0-250Hz 3PH

Short Circuit Rating:65kAIC
Interrupt Capacity Rating:65kAIC
Max. Ambient Temperature: 50°C

Enclosure Type:TYPE 1
Coolant Type:Refrigerant R134a ‘
Design Presure:185 PSIG IIMII |
| il |
| |

Carrier Part Number:19XVA2CC500
VFD Serial Number:41248858
Carrier Dwg. Number:19XR04004501 PRI
DATE 2015/04/28 SALES ORDER NO. 6502365764 / 000101

PLANT 1100
PRODUCT OF USA for Carrier Corporation
Syracuse, NY 13211-4808.
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SER NO 412488568
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