Statement of Work 
1. Purpose and Scope 
· The purpose of this requirement is to procure critical spare parts for the cutter’s Buffalo Pumps ancillary seawater cooling pumps. These parts will provide ship’s force with the necessary components to repair or replace seawater cooling pump parts in the event of mechanical failure.     
2. Deliverables and Performance Requirements
· The vendor shall provide new, unused parts that meet the manufacturer’s specifications and are compatible with the cutter’s ancillary seawater cooling pumps.
· All parts are for Buffalo pump model number AA6CCRE (motor M22H0628RE) and model number 709CCRE (motor M22H0631RE). The listed part numbers are the manufacturer’s part/stock numbers and are provided to identify the required parts. 
· The following are the quantities, manufacturer’s part numbers, and descriptions of the items to be procured. 
	Qty.
	Part No.
	Description

	2
	CC10677-2-267
	Impeller

	4
	15182-17-39
	SFT SLV

	4
	204-29-168
	WRG RNG CSG

	4
	204-29-165
	WRG RNG CSG COV

	4
	231-11-012
	Gasket

	5
	231-11-018
	Gasket

	4
	231-31-1635
	Mech Seal

	2
	CC10677-2-268
	Impeller

	1
	14785--5--252
	Impeller

	1
	14259-6-27
	WRG RNG CSG

	1
	231-11-011
	Gasket Casing

	1
	15137-13-39
	Shaft sleeve


1	231-31-1850			Mech Seal

· Reference 
3. Period of Performance 
· Delivery must be made NLT 01NOV26.
· This requirement is driven by the operational need to procure critical spare parts for the cutter’s Buffalo Pumps ancillary seawater cooling pumps in support of ship readiness following completion of dry dock and prior to winter deployment to Antarctica. The delivery date of NLT 01NOV26 is based on standard commercial lead times, vendor processing, and shipping logistics for specialized pump components. This delivery timeframe reflects typical vendor logistics for sourcing and delivering parts of this type and quantity.

4. Location and Method of Performance 
· USCG Base Seattle, Pier 46F 
1519 Alaskan Way S 
Seattle WA 98134 
5. Roles and Responsibilities 
· Vendor is responsible for delivering parts. 
· Vendor is responsible for all delivery costs. 
· All deliveries must be made to USCG Base Seattle shipping and receiving.  
6. Acceptance Criteria 
The Government will accept the parts if all the following conditions are met:
· Parts are new and unused.
· Parts match the required quantities, part numbers, and descriptions listed in this SOW.
· Parts are compatible with the cutter’s Buffalo Pumps ancillary seawater cooling pumps.
· Parts are free from visible damage or defects.
· Parts are properly packaged to prevent damage during shipment.
· Delivery is made to the required location.
7. Security and Confidentiality 
· Driver must be in possession of Real ID to access USCG Base Seattle. 
8. Reporting Requirements 
· Vendor will provide a receipt with total quantity delivered and price breakdown.
